Version 6.08 (November 6, 2001)
--------------------------------------------------------------------------
This file contains information regarding the corrections, modifications 
and enhancements that have been made since the release of version 6.07.
--------------------------------------------------------------------------

Table of Contents:
1. New Printer Drivers
2. Bugs and Fixes
3. Printer-specific Fixes and Corrections

--------------------------------------------------------------------------

1. NEW PRINTER DRIVERS:
-----------------------

- Kroy K4500
- Pressiza P4083
- Pressiza P4102
- Pressiza P6083
- Pressiza P6102
- Pressiza P8063
- Pressiza P8082
- TEC B852
- TSC Clever TTP-2410


2. BUGS and FIXES:
------------------

- Version 6.08 is fully Windows XP compatible. All previous versions
  of 6.xx support Windows XP but the Hasp security key requires that new
  drivers be installed. These drivers are installed with version 6.08.

- Windows 2000 and Windows NT users are no longer required to have 
  administrator rights to use DDE, ActiveX or Command Files. In previous 
  versions a warning message (Administrator rights required)would appear 
  when starting the program if the user did not have   administration 
  rights. This warning caused problems because a user was not around 
  when the program started to click the OK button to continue.

- Previous versions could not download labels to the PrintPad
  device if used with Windows 2000 or Windows NT. The conflict between 
  PrintPad and the Windows 2000 and Windows NT platforms has been resolved.

- The Print to Picture feature will now create correct JPEG files.

- The MID link expression has been fixed, and will no longer return
  error number 1058.

- Code128 F1 Mod10 will now calculate the check digit based on all the 
  characters in the barcode.  In the past the first 2 digits would be 
  omitted from check digit calculation if the were "00" or "01"
  
- Healthcare version will now recognize network key.

- Linking CommWatch, or When Printed fields to database key field in some cases
  would cause the wrong record to be printed.  This has been resolved.

- DataWatch would produce an "Invalid Bracket" error when monitoring Excel 2000,
  or ODBC text files.  This has been resolved.



3. PRINTER SPECIFIC FIXES AND CORRECTIONS:
------------------------------------------

Bell-Mark
- Adjusted Bell-Mark printer vector font and graphics display position.
- Corrected bug in which larges lines were not printing.

Datamax
- The multiplier of "10" was incorrectly sent for PDF bar codes. The correct
  value of "A" is now sent.

Printronix
- We have optimized print jobs for labels with TrueType fonts or 
  Graphics to print faster.

TEC
- Labels with a TrueType font date field and a decrementing field now 
  optimize print speeds.  
- Print Jobs of 100 labels would send 100 individual jobs. This has 
  been resolved.

Zebra
- Installing the Zebra 90xi III would generate an error message. This 
  has been resolved.
  

=======================================================================
=======================================================================


Version 6.07 (Updated 14 May 2001)
--------------------------------------------------------------------------

NEW FEATURES AND ENHANCEMENTS:
---------------------------------
- Datamax I and W class printers now support High Speed graphics.  
  "High Speed Graphics" option in Label Setup+Options must be selected.  
  In order to use this command the Datamax firmware must be greater than 6.0

- Text and paragraph fields can now include Chinese, Korean and Japanese 
  character sets in Windows 2000.  Chinese, Korean and Japanese fields can 
  be mixed on one label.

- Tec Printers can now at intervals up to 999 labels per batch. Previous 
  versions would only support up to 100 labels.

- Zalton printers can now be used. Previous version required 
  a special security key to use the Zalton printer family.

NEW PRINTER DRIVERS:
-----------------------
Datamax E-4304
Datamax I-4208
Datamax I-4406
Datamax I-4604
Meto mi-4208	
Meto mi-4406
Meto mi-4604
Monarch 9850
Sato 8485/SE 
Sato CX208 DT
Sato CX208 TT
Sato CX212 DT
Sato CX212 TT
Zalton Dandy 4200
Zalton Dandy 4201
Zalton Dandy 4300
Zalton SuperWoven 2-color
Zalton SuperLabel 4
Zalton SuperLabel 5
Zalton SuperLabel 6
Zalton SuperLabel 8
Zalton Super Tag
Zalton SuperWoven 200dpi
Zalton SuperWoven 295dpi
Zalton UltraLabel 4
Zalton UltraLabel 5

PRINTER SPECIFIC FIXES AND CORRECTIONS:
------------------------------------------
Printronix
- T5206 WYSIWYG text problem for large fonts has been corrected.  
- True type font alignment has been improved on all Printronix printers.

Comstar
- Corrected TrueType font printing problem when retrieving data 
  from a database.

Microcom
- Corrected TrueType font printing problem when retrieving data 
  from a database.

C.Ithoh
- Labels with true type fonts are would convert fonts to printer 
  resident when opened in 6.05.  This has been resolved.

=======================================================================
=======================================================================


Version 6.06 (Updated 13 February 2001)
--------------------------------------------------------------------------
NEW FEATURES AND ENHANCEMENTS:
---------------------------------
- No new features have been added to this revision.

NEW PRINTER DRIVERS:
-----------------------
QuickLabel Systems Pronto 442
QuickLabel Systems Pronto 442DT
QuickLabel Systems Pronto 472
QuickLabel Systems Pronto 474
QuickLabel Systems QLS-500
Bell-Mark EasyPrint 2C
Bell-Mark EasyPrint 2CD
Bell-Mark EasyPrint 2F
Bell-Mark EasyPrint 5C
Bell-Mark EasyPrint 5CD
Bell-Mark EasyPrint 5F


PRINTER SPECIFIC FIXES AND CORRECTIONS:
------------------------------------------
Pressiza
- the RSI Prissiza 406 family now supports a temperature ranges of 1-30.
  Previous versions only supported 1-20.

Bell-Mark
- Bell-Mark Drivers are now supported in the Standard product

- Problem with fields being wrapped when being printed on the left edge 
  of EasyPrint 5CD printer has been resolved.

- Pictures/TrueType font positioning is has been improved.

- Gap size can now be specified in 1/100 mm.

=======================================================================
=======================================================================

Version 6.05 (Updated 16 January 2001)
--------------------------------------------------------------------------
NEW FEATURES AND ENHANCEMENTS:
---------------------------------
- New linked functions have been added that allow for entering ASCII
  commands directly into the expression.  For example, the GS function now
  appears on list of linked functions as <GS>, and can be entered as a
  separate field by selecting it off the pull down menu.

- Sato printers have the option to clear the print buffer when printing.
  The clear command, when chosen, will be placed at the beginning of the
  print job and will clear any data stored in the printer.  The option is
  found, when a Sato printer is chosen, on the Edit + Label Setup + Options
  menu.  The default is YES.

- Added support on Eltron printers for the UCC/EAN 128 Multi bar code
  symbology.

- TSC and Intermec printers have an option to clear True Type fonts from
  printer memory with each print job, or to leave downloaded files
  untouched.

- Added a user configurable timeout setting for the Barcode Guardian.  The
  setting is made in the LABEL.INI file and not from within the program.

- When using PDF 417 bar codes, the data source can be set to When Printed
  for control through an external programs. This option is not for use when
  printing directly from the program.

- A new diagnostic reporting feature has been added.  When activated,
  errors generated during an ODBC / OLE DB connection will be logged to a
  file "LVODBCERR.LOG".  This will aid in locating and correcting problems
  with these data sources.

- Added support for mirror imaging on Sato printers.

- A "Continue" button has been added for the Guardian that allows bad
  labels to be ignored, and printing to be continued.

--------------------------------------------------------------------------

NEW PRINTER DRIVERS:
--------------------
Avery Dennison TTK 8
Avery Dennison TTK 12
Citizen CLP-1001
Citizen CLP-2001
Citizen CLP-7001
Citizen CLP-7002
Citizen CLP-7401
C.Itoh S4 Plus
Cognitive Solus II
Comstar Lightning 405
Comstar Lightning 506	
Comstar Lightning 608	
Comstar Lightning 810		
Comstar XXPression
Eltron 2746
Eltron LP 2748
Meto mn-4203
Meto mi-4206
Meto mi-4308
Meto mi-4212
Meto mi-6208
Meto mi-6308
Meto mi-6306
Novexx Texx Tile 200
Novexx Texx Tile 295
Salter S243
Salter S643
Salter S243M
Sato M-8485Se
Sato CL-408e
Sato CL-412e
Sato CL-608e
Sato CL-612e
Sato CT400
Sato CT410
TEC 452 (600dpi)
Zebra 96 Xi III

--------------------------------------------------------------------------


GENERAL FIXES AND CORRECTIONS:
--------------------------------
BAR CODES
- The UCC/EAN128 Multi bar code symbology was not inserting the F1
  character when it needed to for variable AI's.  This has been corrected.

- Corrected a problem where the letters A, B, C, and D were not printing in
  the human readable portion of some bar codes (C39, C128), although they
  were included in the symbology.

- Character data entered will now be preserved where it possible (Code
  128B), and converted to upper case when necessary (Code 39, Code 128A).

- Justification of a bar code using an OLE DB data source printing newly
  added records  is now handled correctly.

- The problem with a bar code moving to the right after printing, using a
  variable field and choosing a value less than the full length allowed by
  the field, has been resolved.

- Fixed an error using Code 128C.  The program will now properly validate
  the length of the data (even number of digits) if the F1 character is
  included.


DATABASE, ODBC, and  OLE DB
- Fixed an error ("1024  not found in database") when selecting a range
  from a database and finding only a single record.

- Printing ranges from an ODBC data file will no longer print repeated
  copies of the last record in the database, but each record will be
  printed correctly.

- Selecting a different Print Field than the Key Field when designing the
  label will no longer cause the "Not found in database" error when
  printing using Quick Print.

- Each picture in an ODBC or OLE database will now be printed correctly,
  not repeating the first picture chosen.

- Corrected a "Not found in database" error occurring if the Key field
  selected was not the first column, and the record chosen to print was not
  the first in the file.

- Selecting multiple copies of multiple records will now print the correct
  quantity of labels with the correct data on each.

- Fixed an issue where the quantity to print was drawn from an ODBC or OLE
  DB data source.  The correct quantities will be printed for each record
  when selecting a range of values.

- Using the Value display mode now shows sample data for ODBC / OLE DB data
  sources and not the generic "ABC".

- Corrected the problem with paragraph fields contained within OLE DB data
  files where the program crashed when going to the Preview window.

- Changing the key field for an ODBC data source will automatically resort
  the data file when printing to keep the browse window synchronized with
  changes to the label.

- Corrected an error printing paragraphs from a database.  If no paragraph
  was specified for a record, another field on the label would be moved
  into the vacant space, and another field would be moved to take its
  place, etc.

- Fixed a problem where choosing records from a database, then selecting a
  range would cause the program to ignore the previously selected records
  when printing.

- A problem with linking a database to a CommWatch field, where none of the
  database information  would be printed, has been fixed.

- Choosing a range of records to print from an ODBC or OLE DB data source
  will now print the correct selected records.

- Fixed a problem when entering a user name and password for a Oracle data
  file would cause an error that the said the entered values were invalid.

- The time taken to begin printing a large range of values from a large
  ODBC data source has been shortened.

- An error was corrected when using an Access data file through OLE DB with
  a numeric only key field, the last digit of the number was being dropped.

- If linking an OLE DB key field to another field on the label, entering
  invalid or blank data in the other field would cause the program to print
  the last good record that was printed. This has been corrected.

- Fixed a problem when linking an OLE DB key field to a When Printed field,
  if no record was entered, or if the record was blank, the last printed
  values were printed on the label.  Now under the same conditions, nothing
  will print in those areas.

- Corrected and error when there were  multiple databases are attached to a
  label, and the quantity is to be drawn from one of them, incorrect record
  information was being printed.

- Selecting multiple ranges from an ODBC database will now print the
  correct quantity of labels.

- Some data was being lost due to incorrect sizing of fields when importing
  data via OLE DB. This problem has been fixed.

- An ODBC Driver error will no longer occur when making multiple changes to
  a label design after printing it.


DATAWATCH
- Corrected an error using Datawatch printing all of the records in an ODBC
  database.  The correct number of labels would print, but all labels would
  show the data from the last record in the file.

- Fixed a problem printing labels through DataWatch using a command line
  where the labels would not print, even though the file was processed.


GRAPHICS
- Designing a label with a variable graphic will no longer crash the
  program if no graphic was selected to print.


JOB MODIFIER UTILITY
- The Job Modifier is not longer editable when using the Runtime / Print
  Only version of the program, in keeping with the intent of Runtime.


LINKED EXPRESSIONS
- The REPT function now correctly accepts and prints 0 repeats of the
  specified item instead of always printing at least 1. Null strings can
  also be used properly.


LABELSELECT
- An error was fixed where having a different printer selected as the
  default for the program than the one the label was designed for caused
  the fonts to be converted and printer settings to revert to default
  values.


MISCELLANEOUS
- Label file names and paths can now be up to 250 characters in length
  without causing errors or program crashes.

- Accessing Quick Printing from a command line will now launch the print
  window if a label is specified.  If no label is specified on the command
  line, then the operator will be able to browse for the label to print.

- File names now accept all appropriate characters for file names.

- Fixed a problem using Command Files and several of the same type of
  printers on different ports.  Changing the port through the Command File
  would route the first label correctly, but the rest would be sent to the
  default printer.

- During installation of the program, the protocol chosen for the parallel
  port will be detected and the appropriate drivers for the security key
  will be installed.

- Temporary files for the program are now created in the program directory,
  allowing for more strict access control by network administrators.

- Corrected a problem where having no printer or a deleted printer listed
  in the LABEL.INI file would delete all of the directory paths setup
  within the program.

- UNDO is now activated for OLE Objects.

- Label files with password protection will not be opened in program
  versions that do not allow passwords.  Access will be denied.

- Setting the sensor to Continuous will eliminate the Vertical Gap setting.
  Changing it back to gap should restore the Vertical Gap option, but this
  did not always happen, leaving the Vertical Gap option grayed out.  This
  has been fixed.

- During installation, if the program is being copied onto an existing
  version, an error will be generated if the old version is in operation.
  If the old version is inactive, the installation will proceed normally.

- Improved checks for circular links.  Program will now detect a circular
  link if a database key field is "Linked" and not "Prompted."

- When processing multiple Command Files, the program would crash if the
  last of these files contained the QuitApp command.  This problem has been
  corrected.


PRINTING
- Corrected an error when trying to print a label designed for a printer
  not on the current computer.  None of the prompts for variable date would
  appear on the Quick Print screen.

- Fixed the problem when printing multiples across, with a run separator
  and serial numbers with multiple copies, where the first label would only
  print one copy before the header.

- Paragraph fields on some printers would print too large and outside the
  expected area (bounding box).  This has been corrected.

- Corrected a problem where a label with an incrementing field, that was
  also using software incrementing, would print the number of copies of
  each number as many times as the quantity entered.

- A problem with erratic incrementing in a bar code using a custom human
  readable field that included spaces has been fixed.  As this is a printer
  issue, we now automatically force a change to Software Incrementing for
  labels that include such a bar code.

- Incrementing with labels across the web would always print the same value
  in the first label. This problem has been addressed.

- Fixed a problem where a label with an incrementing field, set to software
  incrementing, would reset to the printer default settings (speed,
  temperature, etc.) on the second label printed.

- More than one paragraph field on the same label could cause some of the
  paragraphs not to print.  This issue has been resolved.

- Printing graphics from a database will respect the sizing option chosen
  (Fixed Ratio, Stretch to Fit, Do Not Resize).

- Corrected a problem with the label preview where a paragraph, drawn from
  an ODBC data source, would not appear.
--------------------------------------------------------------------------


PRINTER SPECIFIC FIXES AND CORRECTIONS:
------------------------------------------
CAB
- Corrected a problem when printing a label with variable information and
  using software incrementing where the second and subsequent labels
  printed would have the speed and temperature reset to the defaults.


C. ITOH
- Added 3,4, and 5 point Triumvirate font support to the S4-400 DPI.


CODEWRITER
- Added Black Mark sensor type.


COGNITIVE
- Many of these printers have been renamed to conform to Windows standards
  regarding the length of the name.

- Changed the printer setup to reflect the true DPI of the printers (ie.
  203 vs. 200 DPI). Correct values are now used internally when calculating
  positions of fields on the label, and the label dimensions.

- Certain characters (! # @ etc.) at the end of a text field using true
  type fonts will be printed.

- Printer resident font descriptions have been modified to conform to
  manufacturer's standard.

- Fixed a problem when using the resident fonts 8x8 and 9x12.  The wrong
  code was being sent to the printer for these fonts (7x8, 8x12).

- Code 93 bar codes will now print correctly.

- Cognitive has changed the clear memory command from   !# 0 0 0 0   to   !
  0 0 0 0.  Our driver has been modified to keep pace. Printers with new
  firmware will have no problem with the new command.  If your printer has
  older firmware, you must update it, or use the Job Modifier to revert to
  the older command.  Use a script similar to: lines_containing("! 0 0 0
  0") : replace("! 0","!# 0")


DATAMAX
- Label offset values are now validated to be within accepted limits.
  Error messages are generated if an invalid entry is detected.


ELTRON
- Justification of variable fields is now being handled correctly.

- Printing multiples across the web with a serial number created a problem
  with the incorrect quantity being printed, and the incremented field
  would repeat values and skip others.  This problem has been resolved.

- Checks are now being made for valid multiplier values for bar codes.

- Fixed a problem using custom date stamps where the custom file could not
  be chosen.

- UCC/EAN 128 Multi bar code symbology will now correctly encode the F1
  character into the bar code.

- The Duetsch Post bar code will now only accept numeric data.


GENICOM
- Added support for the UCC/EAN128 Multi bar code symbology.


INTERMEC
- The EasyCoder X01 (301, 501, etc.) have been renamed to conform to
  Windows standards.

- Database printing which included the first record would print only the
  first record.  This has been resolved.


MONARCH
- Database printing which included the first record would print only the
  first record.  This has been resolved.


PRINTRONIX
- Label width is now being calculated correctly in 10th's of an inch
  instead of 100th's.  The correct width for labels across the web is also
  calculated correctly.

- Overlapping fields on a label will now print in reverse color (white
  wherever 2 fields cross).  This is standard XOR functionality.

- Maximum speed for the T5208 and the T5306 is now 8ips.

- Corrected an error when printing from a database.  Blank records, or
  fields within a record, will now be left blank when printed, instead of
  repeating the last used information or causing an error.

SATO
- Corrected an error when incrementing and printing multiple labels across
  where the first label would print on top of the last in each row.  The
  correct quantity of labels will also be printed.

- True Type fonts will now print correctly on the 8400RV printer.

- Added support for mirror imaging.

TEC
- Postnet bar codes will now force software incrementing to be enabled.

- Postnet bar codes will no longer cause other fields on the label not to
  print after the first label.

- The B-672 driver now correctly allows labels up to 6.71" wide.

TSC
- Printing multiple labels across the web is now being sent to the printer
  correctly.

- Corrected a problem with counting backwards (negative increment value).


UBI
- Fixed a problem with not printing True Type fonts or graphics.


ZEBRA
- Fixed the form feed command sent to the printer.

=======================================================================
=======================================================================

Version 6.04
-----------------------------------------------------------------------
NEW FEATURES AND ENHANCEMENTS:
-------------------------------
- The maximum length of label and accessory file names is now 255
  characters, database file names can be 31 characters in length.

- 2 new targets and a new action have been added to the Job Modifier
  utility. Line(s)_Containing  and  Append  are now supported functions.

- UCC/EAN 128 Multi now can link to date stamps.  Date stamps must be
  custom date stamps with "Null" spacing option.

- Command files can now accept the Null character for data. ie.
  field_name=""

- The drivers for the HASP security key have been updated to correct some
  problems with Windows NT systems using Service Packs 5 & 6.

- The Eltron TLP2046 printer driver now supports a cutter (Cut every label,
  Don't Cut).

- The label offset range for Eltron printers is now from -99 to 99.

--------------------------------------------------------------------------

NEW PRINTER DRIVERS:
-----------------------
Avery Dennison DPM
Avery Dennison DPM US
Avery Dennison TTK 8
Avery Dennison TTK 12
C. Itoh C4
C. Itoh C4TT
Cognitive DelSol TT
Cognitive DelSol DT
IBM 4400-004(203dpi)
IBM 4400-004(300dpi)
IBM 4400-006(203dpi)
IBM 4400-006(300dpi)
IBM 4400-008(203dpi)
IBM 4400-008(300dpi)
Pitney Bowes J645
Pitney Bowes J693
Pressiza 412-64
Pressiza 512-64
Pressiza 610-64
Pressiza 808-64
Pressiza 408-200
Pressiza 408-300
Pressiza TX408-200
Pressiza TX408-300
Pressiza 406-400
Pressiza 406-400+
Pressiza 406Plus
Zalton Dandy 4401
Zalton UltraLabel 4
Zalton UltraLabel 5
Zalton UltraLabel 6
Zalton UltraLabel 8
Zalton PowerLabel 200
Zalton PowerLabel 295
Zalton SuperWoven 1-color 200
Zalton SuperWoven 1-color 295
Zebra 90 Xi III
Zebra 140 Xi III
Zebra 170 Xi III
Zebra 220 Xi III

--------------------------------------------------------------------------

GENERAL FIXES AND CORRECTIONS:
---------------------------------
DATABASE
- Key field data can no longer be linked to itself.

- Linking bar codes to databases will now check the length of the field to
  ensure that it is correct for the symbology selected.  An error will result
  if the database field length does not match the length required by the
  bar code.


LINKED EXPRESSIONS
- Picture fields can now be properly linked to other fields on the label.
  Linked functions are not supported.

- Barcodes that include control characters (ie. F1) will no longer include
  these in the human readable output even if using customized hr.


MISCELLANEOUS
- Renamed the Zalton SuperWoven printer driver to Zalton 
  SuperWoven 2-color.

- HealthCare version now validates bar code data entered for standards
  compliance.

- If the disk is full, attempts to save labels will generate an error and
  will prevent the labels from being saved to that location.

- Paragraphs set as rotated, or on rotated labels, now maintain uniform and
  correct line spacing.

- Bar codes using a serial file as their data source will now display the
  current value from the serial file on the display instead of 9's as
  placeholders.

- The check digit calculation for Code 128 barcodes that have an even
  number of digits will now no longer include the leading 0 added to pad
  the barcode to an even number of digits including the check digit.

- Selecting No printer will no longer cause an error when using
  LabelSelect.

- Custom human readable fields for barcodes will now center correctly
  beneath the barcode.

- The Print-to-Picure feature now permits the user to "browse" to the
  location to store and name the file.


PRINTPAD
- Scanning input to the PrintPad 500 will now treat alphabetic characters
  correctly.

- Printing UCC/EAN Multi barcodes linked to an incrementing field will now
  increment both the barcode and the human readable portion correctly when
  using the PrintPad.

- PDF 417 barcodes will now correctly support linking to other fields on
  the PrintPad.

- All justification options are now supported on the PrintPad 500.

- Changing file or folder names in Windows will now cause the download
  directory to revert to the root of C:\ if the path was affected by the
  changes.

- The newer BIOS versions for the PrintPad 500 will be recognized by the
  software and it will not try to update it each time.

- Files stored in the root directory (ie. C:\ ) will now download correctly
  without errors.


ODBC DB
- Field lengths from external data files are now sized properly when
  appearing on the label.


OLE DB/OBJECT
- Access databases will now work correctly using Jet 3.51 provider if there
  is an OLE Object also on the label.

- Justification for OLE DB fields now defaults to Left, and changing it is
  also possible.

- OLE DB data sources that contain graphics will no longer crash when
  browsing the database.

- OLE graphics were not printing when using Windows NT operating system.
  This has been corrected.

- Adding an OLE Object to a label will no longer constrain the mouse to a
  limited area once the operation has been completed.


PRINTER SPECIFIC FIXES AND CORRECTIONS:
------------------------------------------
AVERY DENNISON
- Justification issues with rotated fields where a barcode would be shifted
  to the right an amount dependant upon the length of data have been
  corrected.

- The 64XX family of printers now support Code 128 barcodes.

C. ITOH
- Printing a rotated (sideways up or down) barcode with variable data
  linked to fixed data will no longer shift the barcode left or right.


DATAMAX
- Fixed wrong speed settings for the E-4203.


ELTRON
- The label quantity selected will now print correctly when Increment
  Method is set to Printer.

- Printing multiple copies of a serialized number will now print the
  correct quantity of each number, and the correct total quantity.

- Characters in the human readable portion of a barcode will no longer
  overlap.


INTERMEC
- Printing multiple records in a single batch, or using DataWatch to print
  multiple records from a database will print the correct data on the
  label.


MICROCOM
- International characters now print correctly when using the 470 printer.


NOVEXX
- The correct cutter command for the TEXTILE printer is now being used.

- The Chess family of printers now supports Code 128 barcodes.


PRINTRONIX
- PDF 2-D barcodes are now forced into using Software generation to ensure
  that they print correctly.

- Maxicode barcodes are now generated by the software when printing to the
  5206 in order to avoid several firmware issues.

SATO
- Using the Guardian with the 8400RV will now correctly stop the
  printer when the fail conditions have been encountered on the printed
  barcode.

TEC
- Corrected issue with TEC printers using the wrong X-coordinate for
  fields too close to label edge.

- The TEC 416 color printer can now set the interior and exterior colors
  for boxes individually.

=========================================================================
=========================================================================

There was no official release of version 6.03.

=========================================================================
=========================================================================
Version 6.02 (Updated 21 Jan. 2000)
-------------------------------------------------------------------------

NEW FEATURES AND ENHANCEMENTS:
------------------------------
- Custom spacing has been changed to allow greater data transparency.
  Custom spacing is now defined using '*' rather than '9'. As an example, 
  a North American telephone number would be defined as 
  Custom spacing: (***)***-**** Labels designed with 9's in previous 
  versions of the program will be converted.

- Job Modifier now supports null parameters.
  Example: all : replace( "XYZ", "" )

- New commands have been added to the Job Modifier.
  New targets "line_containing" and "lines_containing"
  New action  "append"
  Sample usage:
     Original line:  ^PQ1
     Desired line: ^PQ1,1
     JMS: Line_starting_with("^PQ"),Append(",1")
  The "IF" linked expression now allows a null character.
  Example: IF(FIELD1= "",FIELD2,FIELD3)  
  IE. If TEXT1 is equal to "Null" or "Blank Field" return value of TEXT2
  otherwise return the value of TEXT3.

- Print-to-Picture has been added to command files.

- Bubble help has been added to the Database Editor.

- PrintPad header files have been re-formatted.  The new format allows:
  - more reliable printing
  - more reliable downloads
  - easier implementations of new features
 
- PrintPad enhanced to support OLE objects.
  (The objects are converted to pictures for use on the PrintPad.)

- Access time for databases on network drives has been improved.
--------------------------------------------------------------------------


NEW PRINTER DRIVERS:
-----------------------
Avery 6404            
Avery 6405            
Avery 6406            
Avery 6408            
Avery 350             
Datamax DMX I-4206    
Datamax DMX I-4308    
Datamax DMX ST-3210
Datamax DMX W-6208    
Datamax DMX W-6308    
Datamax DMX W-8306    
Kroy K4350-300dpi     
Kroy K4350-203dpi     
Monarch 9840          
Novexx Chess 4        
Novexx Chess 5        
Novexx Chess 6        
Novexx Chess 8        
Novexx TexxTile 200dpi
Novexx TexxTile 295dpi
Novexx Ocelot 200dpi  
Novexx Ocelot 295dpi  
Novexx Print Engine   
SATO 8490 LH
Sato 8490/S LH
TEC B-482
Zalton Dandy 4200
Zalton Dandy 4201
Zalton Dandy 4300

--------------------------------------------------------------------------

GENERAL FIXES AND CORRECTIONS:
------------------------------
BAR CODE GUARDIAN
- Serials files now update correctly when using the Guardian.

- The Bar Code Guardian no longer crashes the program in Windows NT 4.0

- Label numbers are now reported correctly under all circumstances.

- The Guardian laser is now turned off after all abort conditions.

- Low grade bar codes are now correctly reported as low grade (rather than
  data mismatch).

- Printing status screen and log file now indicate all no-reads and bad
  reads.

- Use Bar Code Guardian checkbox no longer appears on the When Printed
  screen when the Guardian is disabled.

COMMAND FILES
- Command files using external data no longer crash the program if an
  invalid file name is used.

- Printing graphics using run separators and command files has been
  corrected.

- Printing graphics using run separators and DDE has been corrected.

- Print preview is now available through command files.

CUSTOM DATE FORMATS
- Space allocated for long month formats in custom data stamps has been
  corrected.

- Links to custom data files are no longer retained when a custom data is
  changed to a regular date.

- Labels converted from earlier versions no longer search erroneously for a
  custom date file.

DATABASE
- PDF-417 bar codes now print correct data from selected database records.

- Select range using wildcards now consistently prints the correct records.

- When a database key field is changed, the database is now re-sorted in
  the browsing window.
  
LINKED EXPRESSIONS
- AND Linked Expression now returns correct values for true and false
  conditions.

- OR Linked Expression now returns correct values for true and false
  conditions.

- CHR Linked Expression will now correctly accept extended ASCII
  characters.

- TEXT Linked Expression will now accept correct input.

- CYCLENUMBER linked expression using true type fonts now prints correctly.

- The linked expression CHECK128 generates the correct check digit.

PRINTPAD
- PrintPad now supports custom spacing.

- Download status indicator added for the PrintPad 500.

- Incorrect download status correctly reports failed downloads for PrintPad
  500.

- PrintPad now supports longer linked expressions.

- PrintPad warnings for unsupported features enhanced.

- PrintPad now prints UCC/EAN Multi bar codes without errors.

- PrintPad now supports "Must Fill" and "Required" attributes for When
  Printed fields.

- PrintPad now prevents downloading of variable UPC-E barcodes for some
  printers.  This prevents a crash that was occurring. (Printers involved
  are Zebra, Printronix Thermaline, Microcom, Investix, and TopHand2.)

- PrintPad now prints the correct check digit for variable I2of5 
  bar codes (Monarch).

- PrintPad now prints Code 128 bar codes with F1 characters (Printronix
  T5206).

- PrintPad now prints UPC-A human readable code correctly for variable bar
  codes (SATO).

- The <esc> character can now be scanned to navigate screens on the
  PrintPad.

- PrintPad configuration no longer allows configuration of COM3 for the PPD
  1000/2000. (This port does not exist on these models.)
  
ODBC DB
- Bar Codes using ODBC are now updated correctly while printing.

- Paragraphs using ODBC are now updated correctly while printing.

- Fields lengths may now be defined for ODBC data sources.

OLE DB
- When an OLE DB connection is not available, the user is now prompted to
  reestablish the connection upon opening the label.

- OLE DB databases containing OLE objects will no longer crash the program.

- Table names with spaces may now be used with OLE DB.

- OLE DB records may be selected by typing key values.

- Batch printing now consistently prints correct records.

- OLE DB Quantity Data Source now functions correctly when batch printing.

- OLE DB fields may now be used in linked expressions.

- Linked key field definitions now function with OLE DB.

- MSJet 4.0 provider now functions more reliably.

- Define field length now functions for OLE DB.

- Selecting records from the browsing grid is more reliable.

- The prompt property for OLE DB bar codes behaves correctly.

JOB MODIFIER SCRIPT
- Invalid field names in the lines_containing target will no longer cause a
  crash.

- Save button behaves correctly.

OLE OBJECTS
- OLE Objects will retain the correct size after editing.

- Text in OLE Objects is now resized correctly when the object size is
  changed.

- When an OLE source file is not available, the user is now prompted to
  reestablish the connection upon opening the label.

MISCELLANEOUS
- Alpha-numeric incrementing functions correctly when software incrementing
  is used.

- Clear after print will now clear data that have been saved with the
  label.

- Custom Date and Shift Code files have been added to security.

- Custom human readable options are now correct when changing bar code
  symbologies.

- Custom spacing has been increased from 35 characters to 204 characters.

- Default label path is now retained and is more consistent.

- Data Dictionary fields no longer retain a Data Dictionary link when the
  data source is changed.

- Job Modifier now available in Pro Network and Pro Runtime.

- Keyboard Wedge commwatch fields may now accept more than 36 characters of
  data.

- Local (single-user) keys will no longer be detected by installations that
  are set to use a network key.

- Pictures retain the correct size when edited.

- Reset after record now consistently resets to the correct value.

- Quantity data source now works with DataWatch.

--------------------------------------------------------------------------

PRINTER SPECIFIC FIXES AND CORRECTIONS:
---------------------------------------
AVERY DENNISON
- Justification of rotated true type fonts has been corrected.

- F1 linked function now works correctly on Avery printers.

- Sizing and positioning corrected for UPC and EAN bar code with plus
  extensions.

- Vertical Offset has been added.

- 4-digit year date stamps now print the correct century.


C.ITOH
- Offset and backfeed commands have been corrected for the C.ITOH T4

- Speed settings have been corrected for the S4 400dpi.

CAB Apollo1
- Alignment of graphics set as non-resizable has been corrected.

- Some printer resident fonts have been adjusted to display at the correct
  size.

- Human readable code position for the Plessy bar code was has been
  corrected.

COGNITIVE
- Code has been improved to allow more fields to be printed on a Blaster
  Advantage.

- Some printer resident fonts have been adjusted to display at the correct
  size.

DATAMAX
- Batch printing was now works correctly with date or time stamps.

- Print Speed settings for the Allegro 2 are now retained when the label is
  saved and re-opened.

- UCC Shipping Container bar code sizing has been corrected for the 
  Ovation 2.

- UPC and EAN bar code sizing have been corrected for the Ovation 2.

- Justification of the human readable code for Code 128 bar codes has been
  corrected for the Ovation 2.

- Some printer resident fonts have been adjusted to display at the correct
  size for the Ovation 2.

- Code 39 and Code 128 bar codes will now display "A","B" and "C" in the
  human readable code.

- Rotated Italic True Type fonts now print correctly.

- Mirror image has been removed for printers that do not support it.
  (Datamax Allegro, Datamax Allegro 2, Datamax DMX 400, Datamax DMX 430)

ELTRON
- Speed settings for the Eltron LP2423 have been corrected.

- Eltron Stratta driver renamed to Eltron Strata and so no longer crashes
  the program.

- Erase label, graphic, or font for Eltron Printers now functions
  correctly.

- Software generated date formats have been added.

INTERMEC
- Cutter support has been added to the following printers: Intermec 3400C,
  Intermec 4100, Intermec 4240, Intermec 4400, Intermec 4440, Intermec 4630
  Intermec 4830, Intermec 7421
  
- Human readable codes now update correctly when batch printing from a
  database.

MICROCOM
- Cutter options corrected for the Microcom 412.

- Printing of paragraphs has been corrected for the Microcom 412.

- Microcom 412 will now use the full 255 memory slots.

- Print speed increased for the 412 and 466 by the use of binary
  compression for graphics.

MONARCH
- Human Readable codes for Code 128 bar codes have been adjusted on the
  Monarch 9830.

- Labels across will no longer print full rows if not required to on the
  Monarch 9835.

- UPC bar codes over 114% may now be printed on the Monarch 9830.

- Printing labels across has been corrected on the Monarch 9830.

- Printing of paragraphs has been corrected on the Monarch 9830.

- Printing of reversed true type fonts has been corrected on the 
  Monarch 9830.

- Printing of pictures has been corrected.

- Variable paragraphs are no longer required to be filled in order to print
  correctly.

PRINTRONIX
- Bar code sizing and positioning corrected for the PGL-Series

- Code 128 bar codes now print on the PGL-Series

SATO
- Some printer resident fonts have been adjusted to display at the correct
  size for the 8400RV.

- Bar code rotations have been corrected for the CX200.

- Some printer resident fonts have been adjusted to display at the correct
  size for the CX200.

- Bar codes with F1 linked expressions will now print correctly.

- Printing of graphics cleaned up.

TEC
- Incrementing for Codabar bar codes has been corrected.

- Size limitations on scalable fonts are now enforced.

- Brightness and contrast editing is now possible for the TEC CB 416.

TSC
- Some bar codes have been adjusted to display at the correct size for the
  Clever series.

- Bar codes with F1 linked expressions will now print correctly for the
  Clever TTP 243.

ZEBRA
- Print speeds corrected for the Zebra 90xi II/600dpi

==========================================================================
==========================================================================

Version 6.01 (Updated 21 October 1999)

NEW FEATURES:
-------------
- Many of the new features in version 6.0 are briefly described here. For
  more information, check the on-line help.

NEW SECURITY KEY:
- A new security key, the Aladdin HASP key, is replacing the Rainbow keys
  that we have used previously.  This new key has the advantage that it is
  programmable, allowing for easier upgrades.  (We can send you a disk that
  will update the key, rather than replacing the key itself.)

NEW NETWORK SETUP:
- The network setup has been made easier.  Network operation will use
  the License Manager to manage the licenses on all MS Windows platforms.
- Note that network keys will no longer work on a Novell server.

OLE AUTOMATION: [Only available in GOLD version]
- OLE Automation is the technology that is to succeed DDE.  While DDE is
  still supported, new support has been added for OLE Automation. Please
  see installation CD for Visual Basic and C++ samples. A Visual Basic 
  Add-In is also available on the installation CD.

OLE OBJECTS: 
- OLE objects can now be added onto labels.  This means that you can embed
  or link MS Word documents, Clip-art, Word-Art (from MS PowerPoint) in
  your labels.  You can even put sound files on labels!

OLE DB: 
- OLE DB is the technology that is to succeed ODBC. OLE DB is easier to use
  than ODBC, and is more flexible allowing you to use multiple tables from
  your databases.
- Note that, like ODBC, you must install OLE DB Manager (included on
  installation CD) before you can use it.

DIAGNOSTICS:
- A diagnostic screen has been added that will allow you to check your
  configuration at a glance.  Program information, port information, system
  information and library versions are provided on a single screen.
- Diagnostics will also enable you to check your print jobs more easily.
  Print jobs can be configured to be displayed as well as printing to file.
- A bounding box switch enables you (and our test team) to confirm that the
  placement of objects on your labels is truly WYSIWYG. (What you see is
  what you get)
- Diagnostics can be found in the help menu.

CUSTOM HUMAN READABLE:
- Customizing the human readable has been made easier with the addition of
  a Custom Human Readable tab that is available when editing bar codes.

EQUAL SPACING ALIGNMENT:
- A new feature has been added to allow Equal Vertical and Horizontal
  spacing of fields on labels.  More than 2 fields must be selected at one
  time.  The 2 most extreme fields (top and bottom or left and right) will
  not move, but the others will be evenly spaced between these two.

DOWNLOAD TO PRINTPAD:
- A new Windows-based method for downloading files to the PrintPad has been
  added.  Note that you must have PrintPad BIOS 5.31 or better in order to
  use this interface.  Once you have upgraded to this BIOS version, future
  BIOS updates will be done automatically.
- If you do not have this BIOS installed, or if you experience problems
  with the new download interface, you can configure the program to use the
  old download interface by checking the "DOS Download" checkbox in the
  PrintPad tab of the configuration screen. (Options / Configuration /
  PrintPad)

ENHANCED JOB MODIFIER FUNCTIONALITY:
- The job modifier has been enhanced to allow you include field names of
  objects on the label in the syntax of the job modifier.

MISCELLANEOUS:
- A new option has been added to the Command File configuration tab
  (Options + Configuration + Command Files) that will allow users to select
  a prioritization option.  Command files may be executed in order of
  time/date created or alphabetically by file name.  This feature is case
  sensitive;  upper case file names will print before lower case names

------------------------------------------------------------------------

BUG FIXES:
----------
The bug fixes have been categorized, below.  Many of the defects that
have been corrected are printer specific.  These can be found in the
section particular to that printer.


GUARDIAN:
- The Guardian verifier unit gave a no read when scanning Codabar bar
  codes.  This was because of the start and stop characters.  This has been
  corrected.
- When using demand mode on the Guardian verifier, every label in a batch
  used to be entered separately in the log file, but now they are being
  properly combined into their respective batches.
- As the Guardian verifier cannot currently handle ladder orientation for
  bar codes, they are not longer allowed if the Guardian is activated.
- Setting the Laser On/Off buttons for the Guardian will now generate an
  error message if a connection cannot be established.
- The Guardian appeared to be verifying its own warning labels. The syntax
  of the messages given has been changed.
- The Guardian will now correctly verify the F1 character when it is part
  of a linked expression.
- Using a parallel printer with the Guardian would cause approximately 3"
  of label to be printed before the unit was activated.  This will no
  longer happen.


HEALTHCARE VERSION:
- An HIBC barcode could not be printed from the PrintPad if the data was
  drawn from a database. This has been corrected.
- Using HIBCC LIC 128 Secondary barcode (in Healthcare Version) and
  changing the data source to "when printed" now correctly prompts you for
  all three fields required for this type of bar code.
- Corrected a problem linking a text field to an HIBC bar code in the
  Healthcare version.  All that would print out in the text field was the
  opening bracket (.  No data was included.
- Asterisks on HealthCare bar codes will now always be printed in the human
  readable portion regardless of the printer type being used.


ASTROMED:
- Hidden text fields on the Astro-Med Top Hand 2 would disrupt other text
  fields on the label.  This has been fixed.
- A problem using variable data true type fonts where they were not
  correctly represented on the Astro-Med Top Hand 2 Printer has been fixed.
  The fields will now be displayed on the screen as they will be printed.
- The problem with updating fields on labels where there are database
  records printed with True Type Fonts for the Astro-Med Top Hand 2 Printer
  has been corrected.  Incorrect field data was being printed if a large
  range was printed at one time from the database.


AVERY DENNISON:
- Reverse printing (white on black) for the Avery TTX family will now be
  centered properly within the black background.


C.ITOH:
- The error printing from the C.Itoh EZ-4 printer on the PrintPad where
  only a single label was printed has been corrected.


CODEWRITER:
- Reverse printing has been removed from all Codewriter printers as they do
  not readily support this feature.


COGNITIVE:
- A problem printing the Ultra Font b from a Cognitive Solus printer has
  been corrected.  The wrong commands were being used.
- The drivers for the Cognitive Solus printers have been changed to allow
  only 2 printer speeds; 2 and 3 IPS.
- Postnet, Plessey and Code93 barcode symbologies are now available for the
  Cognitive Solus printers.
- The Cognitive (Axiohm) Solus printer drivers now only allow barcode
  rotations of Normal and Sideways Down, as these are the only ones the
  printer supports.


COMSTAR:
- The following new Comstar drivers have been added:
  Comstar Xpression 506 
  Comstar Lightning Jr.
  Comstar Lightning 404
  Comstar Lightning 506 
  Comstar Lightning 607 
  Comstar Lightning 810
  Comstar Color Lightning
  Comstar Color Lightning
  Comstar Color Lightning


DATAMAX:
- The Plessy barcode check digit appears when you print to a Prodigy Max,
  but not when printed on a Prodigy Plus.  This error has been corrected.
- Printing more than 9999 labels using the Datamax Prodigy Max driver
  caused the program to crash. The Datamax Programming Language only
  supports a 4 digit quantity.  The program has been changed such that it
  will no longer crash, but it still won't print 10,000.


ELTRON:
- Some Eltron printers (at least 2642 and 3642) can only file names of 1-8
  characters.  Longer names will cause errors when printing. Label names 
  will now automatically be renamed before being sent to the printer.


INTERMEC:
- The Intermec 4400 printer would return a Range Error 12 or Parameter
  Error 36 when printing graphics or true type fonts.  The printer would
  still print, but the error remained.  The program was passing a value
  which was too small for the data being sent.  It has now been fixed.


MONARCH:
- Label dimensions on the Monarch 9403 were being reversed, since this
  printer loads the label on edge and not flat like most printers.

- Back feeding on the Monarch 9490 Renegade printer is not longer allowed as
  this printer does not support it.


NOVEXX:
- The justification of paragraphs on a NOVEXX would only work correctly for
  some rotations.  This problem has been fixed.


PRINTRONIX:
- Printronix 3306 labels were not displaying as they were printed. This has
  been fixed.
- A bug on the Printronix T3306 printer when using a Code 39 where there
  was a large gap left in the middle of the bar code has been corrected.
  The list of available bar code symbologies has also been changed.
- Paragraph fields printed on the Printronix T4204 can now be resized by
  grabbing the corner of the paragraph and dragging the anchor/handle.
- Several issues with printing rotated fields on a Printronix printer have
  been corrected.


SOABAR:
- An error with Label Logging on Soabar SPX390 printers has been fixed.
  Some fields were being omitted.


TEC:
- The default temperature for a TEC B-572 printer has been restored to 0
  from 10.  The higher setting caused the ribbon to stick to the label and
  tore the ribbon.
- Printing multiple labels across on the TEC 472, 572 or 872 did not print
  correctly.  The number across became the print quantity.  This issue has
  been resolve.
- A printing problem where software incrementing TEXT and a Code 128 Multi
  on the same label caused the fields to overlap on a TEC 572 has been
  fixed.
- Plessey bar code were not printing on the TEC B-572 printer due to
  inconsistent check digits.  Fixed.
- When printing on a TEC printer using center justification and a custom
  human readable field on a bar code, the bar code would be offset to the
  right by approx 1/2 inch.  Fixed.
- Enhancements and improvements to the TEC CB 416 (4 color) printer driver
  have been made.
- True Type fonts were being clipped along the top edge when printing
  rotated on a TEC printer.  Fixed.


TSC:
- Some errors were discovered when trying to print some bar codes that were
  not supported on the TSC Clever printer.  The offending bar code
  symbologies have been removed from those drives to correct the problem.


UBI:
- Continuous and Black mark sensor options have been added for UBI printers.
  Other changes have been made for the UBI line of printers to match
  current printer abilities.


ZEBRA:
- Both the Zebra T-300 and A-300 now support scalable fonts.
- The driver for the Zebra 160S now correctly supports the full 6.3" width
  of the printer.


LINKED EXPRESSIONS:
- A bug was corrected where it was possible to change a field name once
  that name was used in a linked expression. The change can no longer be
  made.
- The linked expression NOW would generate the wrong am/pm value, as well
  as setting the minute to '0' for any actual minute value multiple of 10.
  This has been corrected.
- The CHECKUPCE linked expression will now validate the number of digits
  entered.  Only 6 will be allowed.
- The bug where PrintPad would drop any field using the "ASCII" linked
  function has been fixed.
- Nested IF() expressions could generate syntax and circular link errors on
  some label designs.  Fixed.


DATABASES:
- Databases will now be sorted correctly, instead of not at all, if there
  is a CommWatch field setup to drive the database lookup.
- A label that is printed with just a database and a when printed field
  that increments and is set to "reset after each record" used to have the
  counter stay at the same number if one record is selected. Selecting
  multiple would print correctly.  This has been fixed.
- Test printing with a label using ODBC data sources would force all such
  fields to a size of 10 characters regardless of the actual field length
  specified.  This error has been fixed.
- Text Justification with ODBC data sources would automatically revert to
  left justified when accessing the field a second time regardless of the
  previous setting. Fixed.
- A new feature has been added such that when the user tries to add a
  database field, and there are no dBASE files in the database directory,
  then a browse window will pop-up, allowing the user to change the path
  and select a file.  The new path will be saved as the new default.
- Setting numeric fields with decimals in the database editor was causing
  some problems if 0 decimals was selected.  Now, only 1 number with 0
  decimals, or 3 or more numbers with any decimals will be allowed.
- Adding records in the database editor and then trying to sort by a field
  could cause the new records to be replaced by copies of one of the other
  records.  The further to the right in the database you sort, the more
  fields show up.  This error has been corrected.
- The calculated number of labels to be printed, which appears in Quick
  Print screen after selections from the database have been made, will be
  calculated incorrectly if items were selected and then later deselected.
  Fixed.
- Changing the datasource of the key field of a database would not move the
  key field to another field on the label.  When printing, the database
  browse button was no longer available, preventing data from being
  entered.  This has been fixed.
- Placing more than 205 characters into a memo would cause the program to
  crash when trying to print.  The same database worked fine in earlier
  versions.  This error has been corrected.


GENERAL:
- When printing multiple copies of a label with an incrementing field,
  using a run separator would cause it to print as many times as the number
  of copies selected.  This has been corrected.
- On the Quick Printing Screen, the first variable data field will now be
  highlighted (for easier deletion) rather then the cursor flashing in the
  leftmost position of that text box.
- Some errors were encountered when importing labels from 5.2 where an
  Invalid Page Fault was being generated on the second print job for the
  same label.  This has been fixed.
- There were some problems with "shadow images" appearing on labels
  converted from version 4.2.  The images were not editable, and did not
  print.  The images will no longer appear.
- The displaying of Chinese font problems with the Chinese Version of 
  Windows has been fixed.
- A problem displaying the degree symbol, where it would appear distorted
  on the screen, has been corrected.
- A problem was encountered when moving multiple fields.  When one of the
  fields got close to the edge of the label, it would stop moving while the
  rest continued.  The end result could be to have all of the fields
  aligned to that side of the label, possibly overlapping each other.  This
  has been fixed.
- Using the Erase menu item in would not delete all of the label's files.
  Only the lbl is deleted.  Now, all of the prv, lvd, and ole files are
  removed also.
- When changing the length of serial/database objects, either manually or
  by being incremented, the representation of the object on the screen
  appears cramped or stretched; the number of X's representing the field is
  changed to reflect the new length, but the object size remains the same.
  Printing would always be correct, however.  This problem has been
  corrected.
- Code 128 (multi) with AI=30 will no longer require 8 digits, but will
  allow UP TO 8.
- A problem using a rotated UCC bar code which is placed on a label with a
  text object that has its data source set to database or when printed
  would not print until one of the objects was remove.  This will no longer
  happen.
- The human readable portion of a UCC/EAN 128 (multi) bar code was not
  being properly displayed.  Fixed.
- Numeric only bar codes will now generate a warning if anything other than
  numbers is entered as data.
- Conversion from inches to millimeters would cause would not convert the
  default label properly.  A 4"x2.5" label became a 4mmx2.5mm label. This
  has been corrected to make the conversion to a 101.66mmx63.5mm label as
  it should be.  This error occurred only with the default label.
- A bug when adding a stock to Label Inventory, and then editing the label
  stock would round off the dimensions to the nearest inch.  This has been
  fixed.
- Using CommWatch with a label containing graphics would cause the picture
  to be re-sent with each label, causing slow printing.  Now the graphics
  will only be sent when there has been a change to the image.
- Selecting labels under either Click Print or Quick Print where the
  printer the label was designed for is not the currently selected one
  would cause changes in the setup of the label.  The label would be
  converted to the current printer and its defaults, then back to the
  desired printer and all of its defaults.  The originally established
  parameters will now be maintained.
- The MaxiCode bar code can now print in the 4 standard.
